Building configuration...
!! IOS XR Configuration 6.6.2.10I
!! Last configuration change at Sat Jun  7 17:53:52 2025 by Automation
!
hostname X-RR2
domain vrf mgmt name-server 8.8.8.8
domain vrf mgmt lookup source-interface MgmtEth0/RP0/CPU0/0
domain name dickie.com
domain name-server 8.8.8.8
username pyats
 group netadmin
 password 7 0314420A121C
!
username Automation
 group netadmin
 password 7 06271A354343080D0C181C5A
!
cdp
vrf mgmt
 address-family ipv4 unicast
 !
!
vrf management
 address-family ipv4 unicast
 !
!
line default
 exec-timeout 0 0
 transport input ssh
!
snmp-server vrf management
!
snmp-server host 192.168.122.190 traps version 3 priv snmp
snmp-server host 192.168.122.190 traps version 2c public
snmp-server user snmp SNMPGROUP v3 auth sha encrypted 072E3458463918160443 priv aes 128 encrypted 023616521D360E325F1F
snmp-server user SNMPUSER SNMP-GRP v3 auth md5 encrypted 0448050B1F701E1D priv aes 128 encrypted 08324243194A5746
snmp-server view SNMPVIEW iso included
snmp-server community public RO
snmp-server group SNMPGRP v3 auth read default
snmp-server group LABGROUP v3 auth read default
snmp-server group SNMP-GRP v3 auth read default write default
snmp-server group SNMPGROUP v3 priv read SNMPVIEW
snmp-server traps snmp
snmp-server contact Lab Admin
snmp-server location Rack 1
snmp-server trap-source IPv4 MgmtEth0/RP0/CPU0/0
call-home
 service active
 contact smart-licensing
 profile CiscoTAC-1
  active
  destination transport-method http
 !
!
interface Loopback0
 description Main-Loopback
 ipv4 address 100.0.0.26 255.255.255.255
!
interface MgmtEth0/0/CPU0/0
 vrf mgmt
 ipv4 address 192.168.122.26 255.255.255.0
!
interface GigabitEthernet0/0/0/0
 description link to p2
 cdp
 ipv4 address 1.101.10.2 255.255.255.0
!
interface GigabitEthernet0/0/0/1
 description link to RR1
 cdp
 ipv4 address 1.101.15.2 255.255.255.0
!
interface GigabitEthernet0/0/0/2
 shutdown
!
interface GigabitEthernet0/0/0/3
 shutdown
!
interface GigabitEthernet0/0/0/4
 shutdown
!
interface GigabitEthernet0/0/0/5
 shutdown
!
interface GigabitEthernet0/0/0/6
 shutdown
!
interface GigabitEthernet0/0/0/7
 shutdown
!
router static
 vrf mgmt
  address-family ipv4 unicast
   0.0.0.0/0 192.168.122.1
  !
 !
!
router ospf CORE
 router-id 0.0.0.2
 address-family ipv4 unicast
 area 0
  interface Loopback0
   passive enable
  !
  interface GigabitEthernet0/0/0/0
  !
  interface GigabitEthernet0/0/0/1
  !
 !
!
ssh server v2
ssh server vrf mgmt
ssh server vrf management
end